Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 64 - LIT-18626-13-05
P. 64

    UF4P11E0.book  Page 58  Friday, October 30, 2020  9:39 AM

                            Equipment operation

                            To close the bow storage compartment:
                                                                    Glove compartment:
                            Push the rear of the hood down to securely  Capacity:
                            lock it in place.                           10.2 L (2.7 US gal, 2.2 Imp.gal)
                                                                      Load limit:
                                                                        1.5 kg (3 lb)

                                                                  To close the glove compartment:
                                                                  Push the lid down to securely lock it in place.

                            EJU46000
                            Glove compartment
                            The glove compartment is located in front of
                            the seat.
                            To open the glove compartment:
                            Push the glove compartment latch forward,  To drain water from the glove compartment:
                            and then lift up the lid.             (1) Remove the drain plug on the bottom of
                                                                     the glove compartment to drain the wa-
                                                                     ter.

                                                                                                  1
                                                     1

                              1 Glove compartment latch

                                                                   1 Drain plug
                                                                  (2) Securely install the drain plug in it original
                                                                     position.
                                                                  EJU46011
                                                                  Seat storage compartment
                                                          1       The seat storage compartment is located un-
                                                                  der the rear seat.
                                                                  The storage compartment is removable.

                              1 Glove compartment

                            58

| 59 60 61 62 63 64 65 66 67 68 69 |