Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 97 - LIT-18626-13-05
P. 97

    UF4P11E0.book  Page 91  Friday, October 30, 2020  9:39 AM

                                                                           Care and storage

                            egg, or vegetable oil. Call a physician im-  tends to discharge more quickly if the vehicle
                            mediately.                            is equipped with optional electrical accesso-
                            Eyes: Flush with water for 15 minutes and  ries.  NOTICE: To charge a VRLA  (Valve
                            get prompt medical attention.         Regulated Lead  Acid) battery, a  special
                            Batteries produce explosive gases. Keep  (constant-voltage) battery  charger is  re-
                            sparks, flames, cigarettes, etc., well away.  quired. Using a conventional battery char-
                            If using or charging the battery in an en-  ger will damage the battery. [ECJ02810]
                            closed space, make sure that it is well
                            ventilated. Always shield your eyes when  Checking the battery bands
                            working near batteries.               Make sure  that  the battery bands are  not
                            Keep out of the reach of children.    damaged.

                            To remove the battery:                               1
                            (1) Disconnect the negative (–) battery lead.
                            (2) Disconnect the positive (+) battery lead.
                            (3) Unhook the battery bands, and then re-
                                move the battery from the watercraft.
                                                  1          3
                                                2

                                                                   1 Battery band
                                                                  To store the battery:
                                                                  (1) Clean the battery case using fresh water.
                                                                  (2) If the battery terminals are dirty or cor-
                                                                     roded, clean them using a wire brush.
                              1 Battery band                                       1
                              2 Negative (–) battery terminal: Black lead
                              3 Positive (+) battery terminal: Red lead
                            Checking the battery
                             Make sure that the battery case is not dam-
                              aged.
                             Make  sure that the  battery terminals are
                              not corroded or damaged.
                            Checking the battery voltage and charging
                            the battery
                            It is recommended to have a Yamaha dealer  1 Battery terminal
                            check the battery voltage and charge the bat-  (3) Apply water-resistant grease to the bat-
                            tery. Have a Yamaha dealer charge the bat-  tery terminals.
                            tery as soon as possible if it seems to have
                            discharged. Keep in mind that the battery

                                                                                                   91

| 92 93 94 95 96 97 98 99 100 101 102 |