Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 75 - LIT-18626-13-05
P. 75

    UF4P11E0.book  Page 69  Friday, October 30, 2020  9:39 AM

                                                                    Pre-operation checks

                                      ITEM                         ROUTINE                   PAGE
                             Jet thrust nozzle and re-  Check the jet thrust nozzle and reverse gate for   75
                             verse gate             damage.
                                                    Check the stern drain plugs for damage and foreign
                             Stern drain plugs                                                75
                                                    material and check that they are securely installed.
                             Hood                   Check that the hood is securely closed.   75
                             Front and rear seats   Check that the seats are securely installed.  54
                             POST-LAUNCH CHECKS
                                                    Check that water is discharged from the port (left)
                             Cooling water pilot outlet  cooling water pilot outlet while the engine is run-  75
                                                    ning.
                             Multifunction information   Check the multifunction information center for prop-  76
                             center                 er operation.
                             Shift system           Check the shift system for proper operation.  76
                             Engine idling speed    Check the engine idling speed.            76

                            TIP:
                            To ensure safety and reliability, pre-operation checks should be made each time the water-
                            craft is used.

                                                                                                   69

| 70 71 72 73 74 75 76 77 78 79 80 |