Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 77 - LIT-18626-13-05
P. 77

    UF4P11E0.book  Page 71  Friday, October 30, 2020  9:39 AM

                                                                    Pre-operation checks

                            EJU40182                              nected properly. WARNING! Never operate
                            Engine unit check
                            Check the exterior of the engine unit for dam-  the watercraft if the battery does not have
                                                                  sufficient power to start the engine or if it
                            age or other problem.
                                                                  shows any other signs of decreased pow-
                            EJU36886
                            Engine oil level check                er. Loss of battery power may leave you
                            Make sure that the engine oil level is between  stranded. [EWJ01241]
                            the minimum and maximum level marks on
                            the dipstick. (See page 63 for information on               1  2
                            checking the engine oil level.)

                                                      1

                                                                   1 Negative (–) battery terminal: Black lead
                                                                   2 Positive (+) battery terminal: Red lead
                                                                  Make sure that the battery is securely held in
                              1 Dipstick
                                                                  place.
                                                                  EJU32614
                                                                  Steering system checks
                                                                  Turn the handlebars to the right and left sev-
                                                                  eral times  to  make sure that operation is
                                                                  smooth and unrestricted throughout the
                                                     1            whole range, and that the free play is not ex-
                                                     2            cessive.

                              1 Maximum level mark
                              2 Minimum level mark
                            EJU32456
                            Bilge water check
                            Make sure that no bilge water has collected in
                            the engine compartment. If bilge water has
                            collected in the engine compartment, drain it.
                            (See page 65 for information on draining the
                                                                  Turn the handlebars as far as possible to the
                            bilge water.)
                                                                  right and left to make sure that the jet thrust
                            EJU32486
                            Battery checks                        nozzle moves as the handlebars are turned,
                            Make sure that the battery terminals are not  and that there is no difference between the
                            damaged and that the battery leads are con-

                                                                                                   71

| 72 73 74 75 76 77 78 79 80 81 82 |