Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 49 - LIT-18626-13-05
P. 49

    UF4P11E0.book  Page 43  Friday, October 30, 2020  9:39 AM

                                                                      Watercraft operation

                            The  trim icon  of the home screen is  also  speed can be increased or decreased. How-
                            shown in light yellow.                ever, the adjustment is limited to a maximum
                                                                  of five increments above or below the initial
                              1
                                                                  cruise assist setting.
                                                                  TIP:
                                                                  The cruise assist can only be set between en-
                                            RPM
                                            x1000                 gine speeds of approximately 3000 r/min and
                                                                  approximately 7000 r/min.
                                                   MPH            Activating and deactivating the cruise as-
                                                                  sist
                                                                  Activation of the cruise assist can be con-
                              14.3V
                                                                  firmed by the cruise assist indicator on the
                              1 Trim icon
                                                                  multifunction information center.
                            Locking the drive control mode
                            The drive control mode can be locked.
                            To lock the drive control mode:
                                                                                 RPM
                            (1) Select “Lock”.                                   x1000
                            (2) Input each digit of the 4-digit PIN, and
                                then push the “OK” button of the touch-                 MPH
                                pad control.                                 Cruise Assist  +4
                                                                   14.3V
                                          Enter PIN                              1      2
                                          * * * *                  1 Cruise assist indicator
                                     1       2       3             2 Cruise assist level
                                     4       5       6            To activate the cruise assist:
                                     7       8       9            (1) Operate the throttle lever until the de-
                                             0                       sired engine speed is reached.
                                                                  (2) When the engine speed reaches the de-
                                                                     sired cruise assist  setting, push  the
                            To unlock the drive control mode:        “CRUISE/NO WAKE” switch. Once  the
                            (1) Select the drive control mode indicator.  beeper sounds three times and the
                            (2) Input each digit of the 4-digit PIN, and
                                then push the “OK” button of the touch-
                                pad control.
                            (3) Select “Lock”.
                            EJU45930
                            Cruise assist
                            The cruise assist is a function for maintaining
                            a desired engine speed within a fixed range
                            while  operating the watercraft.  Once the
                            cruise  assist  is activated, the set engine

                                                                                                   43

| 44 45 46 47 48 49 50 51 52 53 54 |