Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 63 - LIT-18626-13-05
P. 63

    UF4P11E0.book  Page 57  Friday, October 30, 2020  9:39 AM

                                                                     Equipment operation

                            could fall, which could result in severe in-  To open the bow storage compartment:
                            jury. [EWJ01511]                      Pull the hood latch rearward, and then lift up
                                                                  the rear of the hood.

                                                                                                 1
                                                         1

                              1 Cleat
                                                                   1 Hood latch
                            EJU31685
                            Storage compartments
                            This watercraft is equipped with the following
                            storage compartments.                             1
                            The storage compartments are not designed
                            to be waterproof.  If you carry objects that
                            must be kept dry, put them in a waterproof
                            bag.
                            Make  sure that  the storage compartments
                            are closed securely before operating the wa-
                            tercraft.
                            EJU45250
                            Bow storage compartment                1 Bow storage compartment
                            The bow storage compartment is located un-
                                                                    Bow storage compartment:
                            der the hood.                             Capacity:
                                                                        92.0 L (24.3 US gal, 20.2 Imp.gal)
                                                                      Load limit:
                                                                        5.0 kg (11 lb)

                                                                                                   57

| 58 59 60 61 62 63 64 65 66 67 68 |