Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 53 - LIT-18626-11-70
P. 53

    UF4D13E0.book  Page 48  Wednesday, March 15, 2017  11:08 AM

                                                                                      Operation

                            A. More throttle produces higher thrust, so  alone using just the amount of thrust
                                the watercraft will turn more sharply.  available at idle.

                            B. Less throttle produces lower thrust, so  D. If the engine is stopped  while riding,
                                the watercraft will turn more gradually.  there is no thrust. The watercraft will go
                                                                     straight even though the handlebars are
                                                                     turned.

                            C. Releasing the  throttle lever completely
                                produces only minimum thrust. If you are
                                traveling  at speeds above trolling,  you  You need throttle to steer.
                                will  have rapidly decreasing ability  to  To maintain  your balance,  lean into a  turn.
                                steer without throttle. You may still have  How much you lean depends on the sharp-
                                some turning ability immediately after re-  ness of the turn and your traveling speed. In
                                leasing the throttle lever, but once the
                                engine slows down, the watercraft will no
                                longer respond to handlebar input until
                                you  apply throttle again or  you reach
                                trolling speed.
                                At trolling speed, the watercraft can be
                                turned gradually by handlebar position

                                                                                                   48

| 48 49 50 51 52 53 54 55 56 57 58 |