Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 56 - LIT-18626-11-72
P. 56

    UF2T17E0.book  Page 51  Thursday, June 22, 2017  3:15 PM

                            Instrument operation

                            DE/RESET” button for less than 1 second.  Tripmeter
                            The display mode changes in the following  This display shows the distance traveled in
                            order.                                kilometers “KM” or miles “MILES” since the
                                                                  measurement was started.

                                                         1

                              1 “MODE/RESET” button
                            Average speed                         Fuel consumption per hour
                            This display shows the average speed in kilo-  This display shows the current fuel consump-
                            meters per hour “AV KMH” or miles per hour  tion in liters per hour “L/HR” or gallons per
                            “AV MPH” since the measurement was start-  hour “G/HR”.
                            ed.

                                                                  Fuel consumption per kilometer/mile
                                                                  This display shows the current fuel consump-
                                                                  tion in liters per kilometer “L/KM” or gallons
                                                                  per mile “G/MILE”.

                            51

| 51 52 53 54 55 56 57 58 59 60 61 |