Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 50 - LIT-18626-11-72
P. 50

    UF2T17E0.book  Page 45  Thursday, June 22, 2017  3:15 PM

                            Instrument operation

                            The large outer numbers on the meter show  then comes on, if “mph” are selected as the
                            the engine speed × 100 rpm (r/min).   display units. (See page 45 for information on
                            The “RPM” indicator light comes on when the  switching the digital speedometer display
                            analog tachometer is selected.        units.)
                            To switch to the tachometer from the speed-
                            ometer:                                1
                            Push the “SPEED/RPM” button for at least 1
                            second after  the multifunction information
                            center is activated. When the meter switches
                            to the analog tachometer function,  the
                            “RPM” indicator light comes on.

                             1                                                                    2
                                                                   1 “SPEED/RPM” button
                                                                   2 “SPEED” indicator light
                                                                  EJU35027
                                                                  Information display
                                                                  The information display shows watercraft op-
                                                                  erating conditions.
                                                             2
                                                                           1     2     3   4
                              1 “SPEED/RPM” button
                              2 “RPM” indicator light
                            Analog speedometer
                            The analog speedometer shows  the water-
                            craft speed against water.
                            The small inner numbers on the meter show
                            the watercraft speed in kilometers per hour
                            “km/h” and the large outer numbers show the       5   6      7
                            speed in miles per hour “mph”.
                                                                   1 Fuel level meter
                            The “SPEED” indicator light comes on when  2 Fuel indicator
                            the analog speedometer is selected.    3 Hour meter/voltmeter
                            To switch to the speedometer from the ta-  4 Digital speedometer
                            chometer:                              5 Engine overheat warning indicator
                            Push the “SPEED/RPM” button for at least 1  6 Check engine warning indicator
                            second after  the multifunction information  7 Oil pressure warning indicator
                            center is activated. When the meter switches  EJU42361
                                                                  Digital speedometer
                            to the analog speedometer function,  the
                                                                  The digital speedometer shows the water-
                            “SPEED” indicator light comes on if “km/h”
                                                                  craft speed against water.
                            are selected  as the display units. The
                            “SPEED” indicator light blinks three  times,

                            45

| 45 46 47 48 49 50 51 52 53 54 55 |