Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 64 - LIT-18626-11-72
P. 64

    UF2T17E0.book  Page 59  Thursday, June 22, 2017  3:15 PM

                            Equipment operation

                            (2) Hook the front of the latch on both sides  Removable beverage holder
                                of the lid onto the hull, and then push the  The removable beverage holder is located in
                                rear of the latch inward to securely lock it  the glove compartment. (See page 57 for in-
                                in place.                         formation on the glove compartment.)
                            TIP:                                     1
                            The ski rope slot in the stern storage com-
                            partment lid can be used to store the rope in
                            the stern  storage compartment while  the
                            rope is attached to the cleat.

                                                                   1 Removable beverage holder
                                1
                                                                  EJU42311
                                                                  Watertight storage compartments
                                                                  This model is equipped with a built-in water-
                                                                  tight storage compartment and a removable
                                                                  watertight storage compartment.
                              1 Ski rope slot
                                                                  These compartments are  watertight when
                            EJU42301                              their caps are closed securely.
                            Beverage holders
                                                                  Built-in watertight storage compartment
                            This model is equipped with a built-in bever-
                                                                  The built-in watertight storage compartment
                            age holder and a removable beverage holder.
                                                                  is located near the port (left) side of the multi-
                            Do not place any items in the beverage hold-
                                                                  function information center.
                            ers while riding. Otherwise, the items may fall
                            out of the beverage holders.
                            Built-in beverage holder
                            The built-in beverage holder is located near
                            the starboard (right) side of the multifunction
                            information center.

                                                          1

                              1 Built-in beverage holder

                            59

| 59 60 61 62 63 64 65 66 67 68 69 |