Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 63 - LIT-18626-11-72
P. 63

    UF2T17E0.book  Page 58  Thursday, June 22, 2017  3:15 PM

                                                                     Equipment operation

                            To close the glove compartment:       EJU42193
                                                                  Stern storage compartment
                            Lower the lid, and then turn the glove com-
                                                                  The stern storage compartment is located in
                            partment knob to securely lock the lid in pla-
                                                                  front of the boarding platform.
                            ce.
                                                                  To open the stern storage compartment:
                                                                  (1) Pull the rear of the stern storage com-
                                                                     partment latch on both sides of the stern
                                                                     storage compartment lid outward,  and
                                                                     then unhook the front of the latch from
                                                                     the hull.

                                                                                              1

                                                                   1 Stern storage compartment latch
                                                                  (2) Open the lid.

                                                                                              2
                            To drain water from the glove compartment:
                            (1) Remove the drain plug on the bottom of
                                the glove compartment to drain the wa-
                                ter.

                                                                           1
                                                                   1 Stern storage compartment lid
                                                                   2 Stern storage compartment
                                  1
                                                                    Stern storage compartment:
                                                                      Capacity:
                                                                        17.0 L (4.5 US gal, 3.7 Imp.gal)
                                                                      Load limit:
                                                                        1.5 kg (3 lb)
                              1 Drain plug
                                                                  To close the stern storage compartment:
                            (2) Securely install the drain plug in its origi-
                                                                  (1) Close the lid.
                                nal position.

                                                                                                   58

| 58 59 60 61 62 63 64 65 66 67 68 |