Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 62 - LIT-18626-11-73
P. 62

    UF3J14E0.book  Page 57  Friday, June 23, 2017  9:47 AM

                            Equipment operation

                            could fall, which could result in severe in-  cleats break, the watercraft could fall,
                            jury. [EWJ01511]                      which could result in severe injury. [EWJ00822]
                                                                  FX Cruiser SVHO
                                                                                               1

                                1

                              1 Cleat
                                                                   1 Pull-up cleat
                            EJU34894
                            Pull-up cleats (FX Cruiser SVHO / FX   FX Limited SVHO
                            Limited SVHO)                                                      1
                            The pull-up cleats are used to attach a rope
                            to the watercraft when mooring it.
                            To use a pull-up cleat, pull it up. The pull-up
                            cleat returns automatically to its original posi-
                            tion when released. WARNING! Do not use
                            the pull-up cleats to lift the watercraft. The
                            pull-up cleats are not designed to support
                            the watercraft’s weight. If the pull-up

                                                                   1 Pull-up cleat
                                                                  EJU42291
                                                                  Storage compartments
                                                                  This watercraft is equipped with the following
                                                                  storage compartments.
                                                                  Only the securely closed watertight storage
                                                                  compartments are waterproof.  If you carry
                                                                  objects that must be kept dry, put them in a
                                                                  waterproof bag.
                                                                  Make sure  that the storage  compartments
                                                                  are closed securely before operating the wa-
                                                                  tercraft.
                                                                  EJU42211
                                                                  Bow storage compartment
                                                                  The bow storage compartment is located un-
                                                                  der the hood.

                            57

| 57 58 59 60 61 62 63 64 65 66 67 |