Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 65 - LIT-18626-11-73
P. 65

    UF3J14E0.book  Page 60  Friday, June 23, 2017  9:47 AM

                                                                     Equipment operation

                            EJU42193                              (2) Hook the front of the latch on both sides
                            Stern storage compartment
                            The stern storage compartment is located in  of the lid onto the hull, and then push the
                                                                     rear of the latch inward to securely lock it
                            front of the boarding platform.
                                                                     in place.
                            To open the stern storage compartment:
                            (1) Pull the rear of the stern storage com-  TIP:
                                partment latch on both sides of the stern  The ski rope slot in the stern storage com-
                                storage compartment lid  outward,  and  partment lid can be used to store the rope in
                                then unhook the front of the latch from  the stern  storage  compartment while the
                                the hull.                         rope is attached to the cleat.

                                                        1

                                                                     1

                              1 Stern storage compartment latch    1 Ski rope slot
                            (2) Open the lid.                     EJU42301
                                                                  Beverage holders
                                                                  This model is equipped with a built-in bever-
                                                         2        age holder and a removable beverage holder.
                                                                  Do not place any items in the beverage hold-
                                                                  ers while riding. Otherwise, the items may fall
                                                                  out of the beverage holders.
                                                                  Built-in beverage holder
                                                                  The built-in beverage holder is located near
                                                                  the starboard (right) side of the multifunction
                                      1                           information center.
                              1 Stern storage compartment lid
                              2 Stern storage compartment                                       1
                              Stern storage compartment:
                                Capacity:
                                  17.0 L (4.5 US gal, 3.7 Imp.gal)
                                Load limit:
                                  1.5 kg (3 lb)

                            To close the stern storage compartment:
                            (1) Close the lid.
                                                                   1 Built-in beverage holder

                                                                                                   60

| 60 61 62 63 64 65 66 67 68 69 70 |