Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 51 - LIT-18626-11-73
P. 51

    UF3J14E0.book  Page 46  Friday, June 23, 2017  9:47 AM

                                                                     Instrument operation

                            By switching the display units, the speed can  the display units are switched from kilome-
                            be shown in kilometers per  hour (km/h) or  ters to miles only, the “SPEED” indicator light
                            miles per hour (mph).                 blinks three times.
                            TIP:
                            Miles are selected as the display units at the  1
                            Yamaha factory.

                                                            1                                     2

                                                                   1 “VOLT/HOUR” button
                                                                   2 “SPEED” indicator light
                                                                  TIP:
                              1 Digital speedometer               The display units can also  be switched by
                            Digital speedometer display (mph)     pushing the “START/STOP” button and
                            The “SPEED” indicator light blinks  three  “MODE/RESET” button simultaneously for at
                            times if miles are selected as the display units  least 8 seconds.
                            when the multifunction information center is
                            activated.
                                                                                               1
                            TIP:
                            If the analog  speedometer  is selected,  the
                            “SPEED” indicator light blinks three  times,
                                                                                               2
                            then comes on.
                            Digital speedometer display (km/h)
                            The “SPEED” indicator light blinks once if ki-
                            lometers are  selected as the display  units
                            when the multifunction information center is
                                                                   1 “START/STOP” button
                            activated.
                                                                   2 “MODE/RESET” button
                            TIP:
                                                                  EJU42261
                            If the analog  speedometer  is selected,  the  Hour meter/voltmeter
                            “SPEED” indicator light blinks once,  then  The hour meter/voltmeter has both an hour
                            comes on.                             meter function and a voltmeter function. By
                            To switch  the  digital speedometer display  switching the meter, it can be used as either
                            units:                                an hour meter or a voltmeter.
                            Push the “VOLT/HOUR” button for at least 1
                            second,  within 10 seconds  after the  multi-
                            function information center is activated. The
                            digital speedometer display changes. When

                                                                                                   46

| 46 47 48 49 50 51 52 53 54 55 56 |