Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 111 - LIT-18626-11-73
P. 111

    UF3J14E0.book  Page 106  Friday, June 23, 2017  9:47 AM

                                                                           Trouble recovery

                                 TROUBLE            POSSIBLE CAUSE             REMEDY         PAGE
                             Watercraft slow or   Watercraft   Low RPM Mode acti-  Deactivate Low RPM
                             loses power      operation   vated           Mode                 40
                                              mode
                                              Cavitation  Jet intake clogged  Clean           107
                                                         Impeller damaged or   Have serviced by   107
                                                         worn             Yamaha dealer
                                              Engine over-  Engine speed reduc-  Clean jet intake and   48
                                              heat warning  tion control activated  cool engine
                                              Oil pressure   Engine speed reduc-  Add oil      48
                                              warning    tion control activated
                                              Spark plug  Fouled or defective  Have serviced by   —
                                                                          Yamaha dealer
                                                         Incorrect heat range  Have serviced by   —
                                                                          Yamaha dealer
                                                         Gap incorrect    Have serviced by     —
                                                                          Yamaha dealer
                                              Electrical wir-  Loose connection  Have serviced by   —
                                              ing                         Yamaha dealer
                                              Fuel       Stale or contaminat-  Have serviced by   —
                                                         ed               Yamaha dealer
                                                         Incorrect octane   Use correct fuel   64
                                                         number
                                              Air filter  Clogged         Have serviced by     —
                                                                          Yamaha dealer
                                                         Oil buildup      Have serviced by     —
                                                                          Yamaha dealer
                                              Throttle lever  Faulty      Have serviced by     —
                                                                          Yamaha dealer

                                                                                                 106

| 106 107 108 109 110 111 112 113 114 115 116 |