Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 52 - LIT-18626-11-73
P. 52

    UF3J14E0.book  Page 47  Friday, June 23, 2017  9:47 AM

                            Instrument operation

                            TIP:                                  Voltmeter
                                                                  The voltmeter shows the battery voltage.
                            The hour meter is  selected at  the  Yamaha
                                                                  When the battery voltage is normal, the volt-
                            factory.
                                                                  meter displays approximately 12 volts.
                                                    1             If the battery voltage has dropped significant-
                                                                  ly, “LO” is displayed on the voltmeter. If the
                                                                  battery voltage has risen significantly, “HI” is
                                                                  displayed. If “LO” or “HI” is displayed, imme-
                                                                  diately return to shore and have a Yamaha
                                                                  dealer service the watercraft.
                                                                  To switch to the voltmeter from the hour me-
                                                                  ter:
                                                                  Push the “VOLT/HOUR” button for at least 1
                              1 Hour meter/voltmeter              second  after the multifunction information
                                                                  center is activated for more than 10 seconds.
                            Hour meter
                                                                  The display  switches  to the voltmeter  from
                            The hour meter shows the total number of
                                                                  the hour meter.
                            hours that the engine has been running since
                            the watercraft was new.
                            TIP:                                   1                   2
                            The elapsed time will be kept even if the bat-
                            tery terminals have been disconnected.
                            To switch to the hour meter from the voltme-
                            ter:
                            Push the “VOLT/HOUR” button for at least 1
                            second after  the multifunction information
                            center is activated for more than 10 seconds.
                            The display switches to the hour meter from  1 “VOLT/HOUR” button
                            the voltmeter.                         2 Voltmeter
                                                                  EJU31515
                                                                  Fuel level meter
                             1                    2               The fuel level meter shows the amount of fuel
                                                                  remaining in the fuel tank. The amount of re-
                                                                  maining fuel  is  shown using eight display
                                                                  segments, which disappear two at a time as
                                                                  the fuel level decreases.

                              1 “VOLT/HOUR” button
                              2 Hour meter

                            47

| 47 48 49 50 51 52 53 54 55 56 57 |