Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 109 - LIT-18626-11-73
P. 109

    UF3J14E0.book  Page 104  Friday, June 23, 2017  9:47 AM

                                                                           Trouble recovery

                            EJU34562
                                                       Troubleshooting
                            If you have any trouble with your watercraft, use the troubleshooting chart to check for the
                            possible cause.
                            If you cannot find the cause, consult a Yamaha dealer.
                            EJU42784
                            Troubleshooting chart
                            Confirm the possible cause and remedy, and then refer to the applicable page.
                                 TROUBLE            POSSIBLE CAUSE             REMEDY         PAGE
                             Engine does not   Yamaha Se-  Lock mode selected  Select unlock mode
                             start (Starter motor   curity System                              31
                             does not turn over)
                                              Engine shut-  Clip not in place  Install clip
                                              off switch                                       32
                                              Fuse       Burned out       Replace fuse and
                                                                          check wiring        109
                                              Battery    Run down         Recharge             94
                                                         Poor terminal con-  Tighten as required
                                                         nections                              94
                                                         Terminal corroded  Clean or replace   94
                                              Starter motor  Faulty       Have serviced by
                                                                          Yamaha dealer        —
                             Engine does not   Throttle lever  Squeezed   Release              32
                             start (Starter motor
                                                         Faulty           Have serviced by
                             turns over)                                                       —
                                                                          Yamaha dealer
                                              RiDE lever  Squeezed        Release              32
                                                         Faulty           Have serviced by
                                                                          Yamaha dealer        —
                                              Fuel       Fuel tank empty  Refill as soon as pos-
                                                                          sible                64
                                                         Stale or contaminat-  Have serviced by
                                                         ed               Yamaha dealer        —
                                              Fuel tank  Water or dirt present  Have serviced by
                                                                          Yamaha dealer        —
                                              Spark plug  Fouled or defective  Have serviced by
                                                                          Yamaha dealer        —
                                              Fuel injec-  Fuel pump faulty  Have serviced by
                                              tion system                 Yamaha dealer        —

                                                                                                 104

| 104 105 106 107 108 109 110 111 112 113 114 |