Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 51 - LIT-18626-11-74
P. 51

    UF2W14E0.book  Page 46  Thursday, June 15, 2017  11:29 AM

                                                                     Instrument operation

                            TIP:
                            The elapsed time will be kept even if the bat-
                            tery terminals have been disconnected.

                                           1
                              1 Hour meter
                            EJU43751
                            Voltmeter
                            The voltmeter shows the battery voltage.
                            When the battery voltage is normal, the volt-
                            meter displays approximately 12 volts.
                            If the battery voltage has dropped significant-
                            ly, “Lo” is displayed on the voltmeter, and the
                            information display, hour meter, and indicator
                            lights turn off. If the battery voltage has risen
                            significantly, “HI” is displayed. If “Lo” or “HI”
                            is displayed, immediately return to shore and
                            have a Yamaha dealer service the watercraft.

                                               1
                              1 Voltmeter

                                                                                                   46

| 46 47 48 49 50 51 52 53 54 55 56 |