Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 84 - LIT-18626-11-74
P. 84

    UF2W14E0.book  Page 79  Thursday, June 15, 2017  11:29 AM

                            Operation

                            (4) Have the first passenger board using the  are securely holding on to the person in
                                same procedure as the operator, place  front of them or to the handgrip provided.
                                their feet on the floor of the footwell, and
                                securely hold on to the operator.

                                                                  (7) Attach the engine shut-off cord (lanyard)
                                                                     to your left wrist, and then attach the clip
                            (5) Have the second passenger  follow the  to the engine shut-off switch.
                                same procedure. When the second pas-  (8) Look  in all directions, start  the  engine,
                                senger is boarding,  try to  balance the  and then start off slowly.
                                watercraft together with the first passen-  EJU33083
                                                                  Starting off
                                ger.
                                                                  EWJ00712
                                                                      WARNING
                                                                  To avoid collisions:
                                                                   Scan constantly for people, objects, and
                                                                   other watercraft. Be alert for conditions
                                                                   that limit your visibility or block your vi-
                                                                   sion of others.
                                                                   Operate defensively at safe speeds and
                                                                   keep a safe distance away from people,
                                                                   objects, and other watercraft.
                                                                   Do not follow directly behind watercraft
                            (6) Make sure that  the passenger(s)  have
                                                                   or other boats. Do not go near others to
                                their feet on the floor of the footwell and
                                                                   spray or splash them with water. Avoid
                                                                   sharp turns or other maneuvers  that
                                                                   make it hard for others to avoid you or
                                                                   understand where you are going. Avoid
                                                                   areas with submerged objects or shal-
                                                                   low water.
                                                                   Take early action to avoid collisions. Re-
                                                                   member, watercraft and other boats do
                                                                   not have  brakes. Do not  release  the
                                                                   throttle lever when trying to steer away

                            79

| 79 80 81 82 83 84 85 86 87 88 89 |