Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 7 - LIT-18626-11-75
P. 7

    UF4G12E0.book  Page 2  Tuesday, August 1, 2017  10:17 AM

                                                          General and important labels

                            EJU30353                              mation on the removable watertight storage
                              Emission control information
                                                                  compartment.)
                            This engine conforms to U.S. Environmental
                            Protection Agency (EPA) and/or California Air
                            Resources Board (CARB) regulations for ma-
                            rine SI engines applicable at the time of man-
                            ufacture.
                            This engine is certified to operate on regular
                            unleaded gasoline.
                            EJU44320
                            Approval label of emission control            1
                            certificate
                            This label is attached to the top of the cylin-
                                                                   1 Emission control information label location
                            der head and to the inside of the engine com-
                            partment. (See page 48 for seat removal and  EMISSION CONTROL INFORMATION
                                                                   THIS ENGINE CONFORMS TO          CALIFORNIA AND U.S. EPA EXHAUST REGULATIONS
                            installation procedures and page 53 for infor-  FOR SI MARINE ENGINES. REFER TO OWNER’S MANUAL FOR MAINTENANCE
                                                                   SPECIFICATIONS AND ADJUSTMENTS.
                                                                   ENGINE FAMILY :  DISPLACEMENT :                                    liters
                                                                   MAX POWER :                                            kW  FEL : HC+NOx               , CO                g/kW-h
                                                                   YAMAHA MOTOR CO.,LTD.
                                                                                         1

                                                                   1 Emission control information label location

                                                                                                    2

| 2 3 4 5 6 7 8 9 10 11 12 |