Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 102 - LIT-18626-11-75
P. 102

    UF4G12E0.book  Page 97  Tuesday, August 1, 2017  10:17 AM

                            Trouble recovery

                                 TROUBLE            POSSIBLE CAUSE             REMEDY         PAGE
                             Watercraft slow or   Watercraft   Low RPM Mode acti-  Deactivate Low RPM
                             loses power      operation   vated           Mode
                                              mode                                             38
                                              (VX Deluxe /
                                              VX Cruiser /
                                              VX Limited)
                                              Cavitation  Jet intake clogged  Clean            98
                                                         Impeller damaged or   Have serviced by   98
                                                         worn             Yamaha dealer
                                              Engine over-  Engine speed reduc-  Clean jet intake and   45
                                              heat warning  tion control activated  cool engine
                                              Oil pressure   Engine speed reduc-  Add oil      45
                                              warning    tion control activated
                                              Spark plug  Fouled or defective  Have serviced by   —
                                                                          Yamaha dealer
                                                         Incorrect heat range  Have serviced by   —
                                                                          Yamaha dealer
                                                         Gap incorrect    Have serviced by     —
                                                                          Yamaha dealer
                                              Electrical wir-  Loose connection  Have serviced by   —
                                              ing                         Yamaha dealer
                                              Fuel       Stale or contaminat-  Have serviced by   —
                                                         ed               Yamaha dealer
                                              Air filter  Clogged         Have serviced by     —
                                                                          Yamaha dealer
                                                         Oil buildup      Have serviced by     —
                                                                          Yamaha dealer
                                              Throttle lever  Faulty      Have serviced by     —
                                                                          Yamaha dealer

                            97

| 97 98 99 100 101 102 103 104 105 106 107 |