Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 74 - LIT-18626-11-76
P. 74

    UF3Y11E0.book  Page 69  Tuesday, May 23, 2017  9:23 AM

                            Operation

                            throttle lever is in the fully closed (idle) posi-  34 for information on operating the shift le-
                            tion.                                 ver.)

                                                                         1

                                                                                2
                                                                   1 Shift lever
                            EX Sport:
                                                                   2 Forward position
                            When the shift lever is in the forward position
                            and the engine is running, the watercraft will
                            move forward. The watercraft will move for-
                            ward at trolling speed even if the throttle lever
                            is in the fully closed (idle) position. (See page

                                                                  EX Deluxe:
                                                                  When the throttle lever is squeezed, the “F”
                                                                  (forward) shift indicator will be displayed and
                                                                  the watercraft will move forward. While the
                                                                  “F” (forward) shift indicator is displayed, the
                                                                  watercraft will move forward at trolling speed
                                                                  even if the throttle lever is in the fully closed

                            69

| 69 70 71 72 73 74 75 76 77 78 79 |