Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 39 - LIT-18626-11-76
P. 39

    UF3Y11E0.book  Page 34  Tuesday, May 23, 2017  9:23 AM

                                                                      Watercraft operation

                            EJU40014                                 will  lower  and the watercraft will  start
                             Watercraft operation functions
                                                                     moving in reverse at trolling speed.
                            EJU40522
                            Reverse system (EX Sport)
                            EWJ01231
                                 WARNING
                                                                        1
                             Do not use the reverse function to slow
                              down or stop the watercraft as it could
                              cause you to lose control, be ejected, or
                              impact the handlebars.
                             Make sure that there are no obstacles or       2  3
                              people behind you before  shifting  into
                                                                   1 Shift lever
                              reverse.
                                                                   2 Reverse position
                             Do not touch the reverse gate while the
                                                                   3 Forward position
                              shift lever is being operated, otherwise
                              you could be pinched.
                            When the shift lever is moved to the reverse
                            position, the reverse gate lowers and deflects
                            the water jet being discharged from the jet  2
                            thrust nozzle. This allows the watercraft to
                            move in reverse.
                            To shift into reverse:                  3
                            (1) Release the throttle lever and let the en-
                                gine speed return to idle.                              1
                            (2) Pull the shift lever rearward until it stops  1 Reverse gate
                                in the reverse position. The reverse gate  2 Forward position
                                                                   3 Reverse position
                                                                  To shift into forward:
                                                                  (1) Release the throttle lever and let the en-
                                                                     gine speed return to idle.
                                                                  (2) Push the shift lever forward until it stops
                                                                     in the forward position. The reverse gate
                                                                     will rise and the watercraft will start mov-
                                                                     ing forward at trolling speed.
                                                                  EJU43154
                                                                  Shift system (EX Deluxe)
                                                                  EWJ01773
                                                                      WARNING
                                                                   Make sure that there are no obstacles or
                                                                   people behind you before  shifting  into
                                                                   reverse.

                                                                                                   34

| 34 35 36 37 38 39 40 41 42 43 44 |