Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 56 - LIT-18626-11-77
P. 56

    UF3P11E0.book  Page 51  Wednesday, June 14, 2017  11:35 AM

                            Equipment operation

                            To close the bow storage compartment:  To open the glove compartment:
                            Return the hood to its original position, and  Pull the glove compartment latch  up,  and
                            then push the hood latch down to securely  then lift up the lid.
                            lock it in place.

                                                                                           1

                                                                   1 Glove compartment latch
                            To drain water from the bow storage com-
                            partment:
                            (1) Remove the drain plug on the bottom of
                                the storage compartment to drain  the
                                water into the engine compartment.                         1

                                                           1

                                                                   1 Glove compartment

                                                                    Glove compartment:
                                                                      Capacity:
                                                                        3.4 L (0.9 US gal, 0.7 Imp.gal)
                                                                      Load limit:
                              1 Drain plug                              1.5 kg (3 lb)
                            (2) Securely install the drain plug in its origi-
                                nal position.
                            EJU43781
                            Glove compartment
                            The glove compartment is located in front of
                            the seat.

                            51

| 51 52 53 54 55 56 57 58 59 60 61 |