Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 122 - LIT-18626-11-77
P. 122

    SportsBoat_F3M12.book  Page 116  Monday, June 12, 2017  11:53 AM

                            Trouble recovery

                                                       Troubleshooting
                            If you have any trouble with your boat, use this section to check for the possible cause. If you
                            cannot find the cause or if the procedure for replacement or repair is not described in this own-
                            er’s/operator’s manual, ask your Yamaha Boat Dealer or a qualified mechanic for the proper
                            service.

                            Troubleshooting chart
                            The Troubleshooting chart contains: “TROUBLE,” “POSSIBLE CAUSE,” “REMEDY,” and
                            “PAGE.”
                            Check the possible cause and remedy, and also the referred page for the maintenance steps
                            to solve the trouble.
                              TROUBLE            POSSIBLE CAUSE                 REMEDY          PAGE
                             Starter mo-  Fuse         Burned out       Replace fuse and check wiring  120
                             tor does not   Battery    Run down         Recharge                106
                             turn over
                                                       Poor terminal con-  Tighten as required  106
                                                       nections
                                                       Battery switch off  Turn on switch        28
                                         Rear platform   Not latched    Latch securely           57
                                         hatch
                                         Starter compo-  Faulty         Have serviced by Yamaha   —
                                         nent                           Boat Dealer
                                         Remote control   Not in neutral posi-  Move remote control lever to   30
                                         lever         tion             neutral position
                             Starter mo-  Engine shut-off   Clip on cord is not in   Install clip in engine shut-off   28
                             tor turns   switch        place            switch
                             over/engine   Fuel        Empty            Refill as soon as possible  72
                             does not                  Stale or contaminat-  Have serviced by Yamaha
                             start                                                               —
                                                       ed               Boat Dealer
                                         Fuel tank     Water or dust collect-  Have serviced by Yamaha   —
                                                       ed               Boat Dealer
                                         Spark plug    Fouled or defective  Have serviced by Yamaha   —
                                                                        Boat Dealer
                                         Crankcase     Filled with fuel  Have serviced by Yamaha   —
                                                                        Boat Dealer
                                                       Filled with water  Have serviced by Yamaha   —
                                                                        Boat Dealer
                                         Fuel filter   Clogged or water col-  Have serviced by Yamaha   —
                                                       lected           Boat Dealer

                            116

| 117 118 119 120 121 122 123 124 125 126 127 |