Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 14 - LIT-18626-12-09
P. 14

    UF4D14E0.book  Page 9  Tuesday, March 27, 2018  1:02 PM

                                Safety information

                              (paralysis), facial injuries, and broken legs,  colliding with another boat, which could re-
                              ankles,  and other bones.  Do not jump  sult in severe injury or death.
                              wakes or waves.
                             Do not operate the watercraft in rough wa-
                              ter, bad weather, or when visibility is poor;
                              this may lead to an accident causing injury
                              or death. Be alert to the possibility of ad-
                              verse weather. Take note of weather fore-
                              casts  and  the  prevailing  weather
                              conditions before setting out on your wa-
                              tercraft.
                             As with any water sport, you should not op-
                              erate your watercraft without someone else   Follow navigation rules, and state/provin-
                              nearby. If you operate further than swim-  cial and local laws that apply to watercraft.
                              ming distance from shore, you should be
                              accompanied by  another boat or water-
                              craft, but make sure you stay a safe dis-
                              tance away. It’s good, common sense.
                             Never operate in water that is less than 60
                              cm (2 ft) deep from the bottom of the wa-
                              tercraft, otherwise you increase your chan-
                              ce  of hitting a submerged object,  which
                              could result in injury.

                             This watercraft is not equipped with light-
                              ing required for night operation. Do not op-
                              erate the watercraft after sunset or before
                              dawn, otherwise you increase  the risk of

                            9

| 9 10 11 12 13 14 15 16 17 18 19 |