Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 73 - LIT-18626-12-09
P. 73

    UF4D14E0.book  Page 68  Tuesday, March 27, 2018  1:02 PM

                                                                           Trouble recovery

                            EJU34562
                                                       Troubleshooting
                            If you have any trouble with your watercraft, use the troubleshooting chart to check for the
                            possible cause.
                            If you cannot find the cause, consult a Yamaha dealer.
                            EJU34576
                            Troubleshooting chart
                                 TROUBLE            POSSIBLE CAUSE             REMEDY         PAGE
                             Engine does not   Engine shut-  Clip not in place  Install clip
                             start (Starter motor   off switch                                 23
                             does not turn over)
                                              Fuse       Burned out       Replace fuse and
                                                                          check wiring         71
                                              Battery    Run down         Recharge             55
                                                         Poor terminal con-  Tighten as required
                                                         nections                              55
                                                         Terminal corroded  Clean or replace   55
                                              Starter motor  Faulty       Have serviced by
                                                                          Yamaha dealer        —
                             Engine does not   Fuel cock  Turned to “OFF”  Turn fuel cock knob
                             start (Starter motor                         to “ON”              25
                             turns over)
                                              Fuel       Empty            Refill as soon as pos-
                                                                          sible                32
                                                         Stale or contaminat-  Have serviced by
                                                         ed               Yamaha dealer        —
                                              Fuel tank  Water or dirt present  Have serviced by
                                                                          Yamaha dealer        —
                                              Spark plug  Fouled or defective  Replace         64
                                              Spark plug   Not connected or   Connect properly
                                              cap        loose                                 64
                                              Crankcase  Filled with water  Have serviced by
                                                                          Yamaha dealer        73
                                              Fuel filter  Clogged or water   Have serviced by
                                                         pooled           Yamaha dealer        65
                                              Choke      Knob moves back on  Tighten choke knob
                                                         its own          adjusting nut        65

                                                                                                   68

| 68 69 70 71 72 73 74 75 76 77 78 |