Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 62 - LIT-18626-12-10
P. 62

    UF3V10E0.book  Page 57  Thursday, August 23, 2018  9:17 AM

                            Equipment operation

                            when released. WARNING! Do not use the  EJU34873
                                                                  Bow eye
                            reboarding step to lift the watercraft. The
                                                                  The bow eye is used to attach a rope to the
                            reboarding step is not designed to support
                                                                  watercraft  when transporting, mooring, or
                            the watercraft’s weight. If the reboarding
                                                                  towing it in an emergency. (See page 110 for
                            step  breaks,  the watercraft could fall,
                                                                  information on towing the watercraft.)
                            which could result in severe injury. [EWJ01212]

                              1
                                                                      1

                                                                   1 Bow eye
                              1 Reboarding step
                                                                  EJU34882
                                                                  Stern eyes
                                                                  The stern eyes are used to attach a rope to
                                                                  the watercraft when transporting or mooring
                                                                  it.

                            ECJ00743
                             NOTICE
                                                                        1
                            Use the reboarding step only to board the                            1
                            watercraft in the water. Do not use the re-
                            boarding step for any other purpose. The  1 Stern eye
                            watercraft can be damaged.            EJU40423
                                                                  Cleat
                                                                  The cleat is used to attach a ski rope to the
                                                                  watercraft  when pulling a wakeboarder or
                                                                  water-skier.  WARNING! Do not use the
                                                                  cleat to lift the watercraft. The cleat is not
                                                                  designed to support the watercraft’s
                                                                  weight. If the cleat breaks, the watercraft

                            57

| 57 58 59 60 61 62 63 64 65 66 67 |