Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 108 - LIT-18626-12-10
P. 108

    UF3V10E0.book  Page 103  Thursday, August 23, 2018  9:17 AM

                            Trouble recovery

                            EJU34562
                                                       Troubleshooting
                            If you have any trouble with your watercraft, use the troubleshooting chart to check for the
                            possible cause.
                            If you cannot find the cause, consult a Yamaha dealer.
                            EJU45390
                            Troubleshooting chart
                            Confirm the possible cause and remedy, and then refer to the applicable page.
                                 TROUBLE            POSSIBLE CAUSE             REMEDY         PAGE
                             Engine does not   Yamaha Se-  Lock mode selected  Select unlock mode
                             start (Starter motor   curity System                              31
                             does not turn over)
                                              Engine shut-  Clip not in place  Install clip
                                              off switch                                       32
                                              Fuse       Burned out       Replace fuse and
                                                                          check wiring        108
                                              Battery    Run down         Recharge             93
                                                         Poor terminal con-  Tighten as required
                                                         nections                              93
                                                         Terminal corroded  Clean or replace   93
                                              Starter motor  Faulty       Have serviced by
                                                                          Yamaha dealer        —
                                              Throttle lever  Squeezed    Release              32
                                                         Faulty           Have serviced by
                                                                          Yamaha dealer        —
                                              RiDE lever  Squeezed        Release              32
                                                         Faulty           Have serviced by
                                                                          Yamaha dealer        —
                             Engine does not   Fuel      Fuel tank empty  Refill as soon as pos-
                             start (Starter motor                         sible                63
                             turns over)
                                                         Stale or contaminat-  Have serviced by
                                                         ed               Yamaha dealer        —
                                              Fuel tank  Water or dirt present  Have serviced by
                                                                          Yamaha dealer        —
                                              Spark plug  Fouled or defective  Have serviced by
                                                                          Yamaha dealer        —
                                              Fuel injec-  Fuel pump faulty  Have serviced by
                                              tion system                 Yamaha dealer        —

                            103

| 103 104 105 106 107 108 109 110 111 112 113 |