Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 57 - LIT-18626-12-10
P. 57

    UF3V10E0.book  Page 52  Thursday, August 23, 2018  9:17 AM

                                                                     Instrument operation

                            Displaying the time since the last mainte-   Total fuel used: 0.0
                            nance (“Wellness”)
                            The total number of hours that the engine has
                            been running since the last watercraft main-
                            tenance can be displayed.                          Reset To
                                                                              Factory?

                                     Time Since Last                             Reset
                                       Maintenance

                                        30.0Hrs
                                           Reset                  To reset  the settings, trip information, and
                                                                  fuel information:
                                                                  (1) Tap the “Reset” button.
                                                                  (2) Tap the “YES” button in the confirmation
                            To reset the number of hours of operation:  screen.
                            (1) Tap the “Reset” button.           EJU45190
                                                                  Engine lock screen “   ”
                            (2) Tap the “Confirm Reset” button to reset
                                                                  The engine lock  screen shows the  setting
                                the number of hours of operation.
                                                                  screen for the Yamaha Security System in the
                            Resetting the settings, trip information,
                            and fuel information (“Reset”)        center display. (See page 31 for Yamaha Se-
                            The settings, trip information, and fuel infor-  curity System setting procedures.)
                            mation can be reset to their factory default  EJU45201
                                                                  Warning function
                            settings. The items that are reset and the de-
                                                                  The multifunction information center can indi-
                            fault settings are as follows.
                                                                  cate the following warnings.
                             Display units: US Unit
                                                                   Fuel level warning
                             Language: English
                                                                   Battery voltage warning
                             Display brightness: 100%
                                                                   Check engine warning
                             Color setting: Blue
                                                                   Engine overheat warning
                             Trip time: 0.0
                                                                   Oil pressure warning
                             Distance traveled: 0.0
                                                                   Other warnings (communication errors, ex-
                             Average fuel consumption per gallon or li-
                                                                   ceeding the maintenance intervals, and so
                              ter: 0.0
                                                                   on)
                                                                  To stop the buzzer when a malfunction is ac-
                                                                  tivated, correct the cause of the problem and

                                                                                                   52

| 52 53 54 55 56 57 58 59 60 61 62 |