Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 52 - LIT-18626-12-10
P. 52

    UF3V10E0.book  Page 47  Thursday, August 23, 2018  9:17 AM

                            Instrument operation

                            EJU45121                              symbol in the warning bar that is displayed
                            Operation buttons
                                                                  when a warning is activated.
                            This model is equipped with operation but-
                            tons that can be used in addition to touching          1
                            the multifunction information center.

                                             1      2                                      MPH
                                                                    0                           100%

                                                                     13.6V           x100       N
                                                                                     RPM
                                                                                   2
                                                                   1 Screen tab bar
                              1 “MENU SCROLL” button               2 Center display
                              2 “ALARM MUTE” button
                            “MENU SCROLL” button
                            Each time this button is pushed, the multi-
                            function information center switches in the
                            following order.                                       1
                            Home screen → Information screen (“Trip In-  1 Warning bar
                            fo”)  →  Information screen (“Fuel Info”)  →
                                                                  Screen tab bar
                            Home screen
                                                                  When each symbol is tapped, the watercraft
                            “ALARM MUTE” button                   information, function settings, and other in-
                            Push this button to stop the buzzer when a
                                                                  formation are shown  in the center display.
                            warning is activated. If this button is pushed
                                                                  (See page 48 for information on each screen.)
                            again while the warning is still activated, the
                                                                  Center display
                            buzzer will start sounding again.
                                                                  The center display shows the watercraft in-
                            TIP:                                  formation, function settings, and other infor-
                             The operation sounds cannot be turned off.  mation according  to the symbol on  the
                             If the “ALARM MUTE” button was pushed  screen tab bar that is tapped.
                              to stop the buzzer, the buzzer will  start  Warning bar
                              sounding again after 5 minutes.     The warning bar is shown instead of the ta-
                            EJU45131                              chometer value display only when an error or
                            Touch screen
                                                                  malfunction is detected.
                            The touch operations are enabled only for the
                                                                  When the  warning symbol is tapped,  the
                            screen tab bar, the items and sliders that are
                                                                  warning description, error code, and other in-
                            shown in the center display, and the warning
                                                                  formation are shown  in the center display.
                                                                  (See page 52 for information about the warn-
                                                                  ing descriptions.)

                            47

| 47 48 49 50 51 52 53 54 55 56 57 |