Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 51 - LIT-18626-12-11
P. 51

    UF3X10E0.book  Page 46  Tuesday, August 7, 2018  2:42 PM

                                                                     Instrument operation

                            EJU45110                               While  pushing the engine stop switch,
                                Multifunction information
                                                                   push the start switch.
                                          center                  Turning off the multifunction information
                            The multifunction information center displays  center
                            various watercraft information.       If the multifunction information center does
                            The multifunction information  center is a  not receive any operation input within 25 sec-
                            touch screen that you can touch directly to  onds after the engine stops or if 3 minutes
                            turn the various functions on or off or change  has elapsed after the engine stops, the center
                            settings.                             turns off.
                            In  addition, the language and display units  TIP:
                            shown can be changed. (See page 50 for in-  The multifunction information center turns off
                            formation on changing the language and dis-  3 minutes after the engine stops even if there
                            play units.) In the illustrations in this manual,  is operation input.
                            English is used for the language and US units  Message indicating that operation input
                            are used for the display units.       cannot be received
                            EWJ01980
                                                                  If “Turn OFF Engine”, “Engine Comm Error”,
                                 WARNING
                                                                  or other message appears in red characters
                            For safety, do not touch the multifunction  during touch  operation, the operation  input
                            information center while the watercraft is  cannot be received because the input condi-
                            moving. Otherwise, you could lose control  tions are not satisfied.
                            of the watercraft, which may lead to an ac-  Perform the operation again according to the
                            cident.                               displayed message, or stop the engine to
                                                                  turn off the multifunction information center,
                            TIP:
                                                                  and then turn on the center again. If the mes-
                            The multifunction information center does not
                                                                  sage remains displayed, consult a Yamaha
                            receive operation input while the watercraft is
                                                                  dealer.
                            moving. Before operating the multifunction
                            information center, stop the  watercraft  and
                            check the area around you to make sure it is  Turn OFF Engine
                            safe to operate the center.
                            Turning on the multifunction information        ON          OFF
                            center
                            When the start switch is pushed, the multi-
                                                                                 Save
                            function information center turns on. After the
                            logo display appears for a few seconds, the
                            home screen is displayed  and the touch
                            screen can be operated by touching it.
                            TIP:
                            Perform  one of the following operations  to
                            turn on the multifunction information center
                            without starting the engine.
                             Push the start switch briefly.

                                                                                                   46

| 46 47 48 49 50 51 52 53 54 55 56 |