Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 8 - LIT-18626-12-11
P. 8

    UF3X10E0.book  Page 3  Tuesday, August 7, 2018  2:42 PM

                            General and important labels

                            gine cover removal  and installation  proce-  Watercraft and Outboard marine engine 2001
                            dures.)                               exhaust emission standards. Engines meet-
                                                                  ing these standards have 75% lower emis-
                                                                  sions than conventional carbureted two-
                                                                  stroke engines. These engines are equivalent
                                   1
                                                                  to the U.S. EPA’s 2006 standards for marine
                                                                  engines.

                              1 Manufactured date label location

                                                                  Two Stars - Very Low Emission
                                                                  The two-star label  identifies engines  that
                                                                  meet the Air Resources Board’s Personal
                                                                  Watercraft and Outboard marine engine 2004
                                                                  exhaust emission standards. Engines meet-
                                                                  ing these standards have 20% lower emis-
                            EJU30441                              sions than One Star-Low Emission engines.
                            Star labels
                            This watercraft is labeled with a California Air
                            Resources Board (CARB) star label. See be-
                            low for a description of your particular label.

                                                           1

                                                                  Three Stars - Ultra Low Emission
                                                                  The three-star label identifies engines that
                                                                  meet the Air Resources Board’s Personal
                                                                  Watercraft and Outboard marine engine 2008
                              1 Star label location
                                                                  exhaust emission standards or the Sterndrive
                            One Star - Low Emission               and Inboard marine engine 2003-2008 ex-
                            The one-star label identifies engines that
                                                                  haust emission standards. Engines meeting
                            meet the Air Resources Board’s Personal

                            3

| 3 4 5 6 7 8 9 10 11 12 13 |