Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 51 - LIT-18626-12-16
P. 51

    UF3Y12E0.book  Page 46  Friday, April 27, 2018  1:38 PM

                                                                     Equipment operation

                            towing it in an emergency. (See page 98 for  could fall, which could result in severe in-
                            information on towing the watercraft.)  jury. [EWJ01511]

                                                                                                 1

                              1
                              1 Bow eye                            1 Cleat
                            EJU34882                              EJU31685
                            Stern eyes                            Storage compartments
                            The stern eyes are used to attach a rope to  This watercraft is equipped with the following
                            the watercraft when transporting or mooring  storage compartments.
                            it.                                   The storage compartments are not designed
                                                                  to be waterproof.  If you carry objects that
                                                                  must be kept dry, put them in a waterproof
                                                                  bag.
                                                                  Make sure  that the storage  compartments
                                                                  are closed securely before operating the wa-
                                                                  tercraft.
                                                                  EJU44660
                                                                  Bow storage compartment
                                                                  The bow storage compartment is located un-
                               1                                  der the hood.
                              1 Stern eye
                            EJU40423
                            Cleat
                            The cleat is used to attach a ski rope to the
                            watercraft  when pulling a  wakeboarder or
                            water-skier.  WARNING!  Do not use the
                            cleat to lift the watercraft. The cleat is not
                            designed to support the watercraft’s
                            weight. If the cleat breaks, the watercraft

                                                                                                   46

| 46 47 48 49 50 51 52 53 54 55 56 |