Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 50 - LIT-18626-12-16
P. 50

    UF3Y12E0.book  Page 45  Friday, April 27, 2018  1:38 PM

                            Equipment operation

                            breaks, the watercraft could fall, which  step breaks, the watercraft  could  fall,
                            could result in severe injury. [EWJ00022]  which could result in severe injury. [EWJ01212]

                                                                                               1
                                                           1

                              1 Handgrip                           1 Reboarding step
                            EJU37382
                            Reboarding grip
                            The reboarding grip is used when boarding
                            the watercraft from the water.

                                                           1

                                                                  ECJ00743
                                                                  NOTICE
                                                                  Use the reboarding step only to board the
                              1 Reboarding grip                   watercraft in the water. Do not use the re-
                                                                  boarding step for any other purpose. The
                            EJU34865
                            Reboarding step (EX Sport / EX        watercraft can be damaged.
                            Deluxe)
                                                                  EJU34873
                            The reboarding step is used to assist in re-  Bow eye
                            boarding the watercraft from the water.  The bow eye is used to attach a rope to the
                            When boarding the watercraft, push the re-  watercraft  when transporting, mooring, or
                            boarding step down until it stops. The step
                            returns automatically to its original position
                            when released. WARNING! Do not use the
                            reboarding step to lift the watercraft. The
                            reboarding step is not designed to support
                            the watercraft’s weight. If the reboarding

                            45

| 45 46 47 48 49 50 51 52 53 54 55 |