Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 67 - LIT-18626-12-56
P. 67

    Maintenance

           EJU41751                             ways carry it with you whenever you use the
                     Maintenance
                                                watercraft.
           Periodic  checks and  lubrication will keep
           your watercraft in the safest and most effi-
           cient condition  possible. Therefore, make
           sure to carry out the periodic maintenance.
           Safety is an obligation of the watercraft own-
           er. The most important points of watercraft
           inspection and lubrication are explained on
           the following pages.
           See a Yamaha dealer for genuine Yamaha re-
           placement parts and  optional accessories
           designed for your watercraft.          1 Tool bag
           EWJ00312                               2 Screwdriver
               WARNING                            3 10/12 mm box wrench
           Be sure to turn off the engine when you  4 Spark plug (one included for each cylinder)
           perform maintenance  unless otherwise  5 14/21 mm box wrench
           specified. If you are not familiar with ma-  6 Pliers
                                                  7 10/12 mm open-end wrench
           chine servicing, this work should be done
           by a Yamaha dealer or other qualified me-  EJU34338
                                                Adjusting the steering friction
           chanic.
                                                The amount of friction in the steering can be
           A service  manual is  available for  purchase  adjusted to suit operator preference.
           through a  Yamaha dealer  for owners  who  To adjust the steering friction:
           have the mechanical skills, tools, and other  (1) Lift the steering pole and support it with
           equipment necessary to perform  mainte-  the lock pin.
           nance not covered by this owner’s/operator’s
           manual.
           EJU33803
           Tool kit
           A tool  kit is included with this watercraft.
           Place the tool kit in a waterproof bag and al-

                                                  1 Steering pole
                                                  2 Lock pin

                                                                                 60

| 62 63 64 65 66 67 68 69 70 71 72 |