Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 75 - LIT-18626-12-56
P. 75

    Trouble recovery

           EJU34562
                                      Troubleshooting
           If you have any trouble with your watercraft, use the troubleshooting chart to check for the
           possible cause.
           If you cannot find the cause, consult a Yamaha dealer.
           EJU34576
           Troubleshooting chart
               TROUBLE             POSSIBLE CAUSE            REMEDY         PAGE
           Engine does not   Engine shut-  Clip not in place  Install clip
           start (Starter motor   off switch                                 22
           does not turn over)  Fuse    Burned out       Replace fuse and
                                                         check wiring        71
                            Battery     Run down         Recharge            55
                                        Poor terminal con-  Tighten as required
                                        nections                             55
                                        Terminal corroded  Clean or replace  55
                            Starter motor  Faulty        Have serviced by
                                                         Yamaha dealer       —
           Engine does not   Fuel cock  Turned to “OFF”  Turn fuel cock knob
           start (Starter motor                          to “ON”             24
           turns over)      Fuel        Empty            Refill as soon as pos-
                                                         sible               31
                                        Stale or contaminat-  Have serviced by
                                        ed               Yamaha dealer       —
                            Fuel tank   Water or dirt present  Have serviced by
                                                         Yamaha dealer       —
                            Spark plug  Fouled or defective  Replace         64
                            Spark plug   Not connected or   Connect properly
                            cap         loose                                64
                            Crankcase   Filled with water  Have serviced by
                                                         Yamaha dealer       73
                            Fuel filter  Clogged or water   Have serviced by
                                        pooled           Yamaha dealer       65
                            Choke       Knob moves back on  Tighten choke knob
                                        its own          adjusting nut       65

                                                                                 68

| 70 71 72 73 74 75 76 77 78 79 80 |