Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 16 - LIT-18626-12-57
P. 16

    UF3P13E0.book  Page 10  Monday, June 24, 2019  1:32 PM

                                Safety information

                            EJU30675                              EJU30733
                                                                      Limitations on who may
                            The safe use and operation of this water-  operate the watercraft
                            craft is dependent upon the use of proper   Make sure that the operator is 16 years of
                            riding techniques, as well  as  upon  the  age or older and has taken a boater safety
                            common sense, good judgment, and ex-   course.
                            pertise  of the  operator. Every operator  Adults must supervise use by minors.
                            should  know the following requirements  Your state (or province) may have addition-
                            before riding the watercraft.          al requirements. You can find local rules by
                             Before operating the watercraft, read this  contacting the United States Coast Guard
                              owner’s/operator’s manual,  the Riding  (USCG), the National Association of State
                              Practice Guide, the Riding Instruction card,  Boating Law Administrators, or your local
                              and all labels on the watercraft. Also, watch  Power Squadron.
                              the WaveRunner Basic Orientation Video   This watercraft is designed to carry the op-
                              linked to the following QR code.     erator and up to 2 passengers. Never ex-
                                                                   ceed the maximum load limit or allow more
                                                                   than  3 persons  (or 2  persons if a wake-
                                                                   boarder or water-skier is being pulled) to
                                                                   ride the watercraft at any time.

                              https://yamahawaverunners.com/orientation
                              A DVD is also  available  at your  nearest
                              dealer for your convenience.
                              These materials should give you an under-
                              standing of the watercraft and its opera-
                                                                    Maximum load:
                              tion.
                                                                      240 kg (530 lb)
                             Never allow anyone to operate this water-  Load is the total weight of cargo, op-
                              craft  until they  too have read this own-  erator, and passengers.
                              er’s/operator’s manual, the Riding Practice
                              Guide, the Riding Instruction card, and all   Do not operate the watercraft with any pas-
                              labels, and,  if  possible, watched the  sengers on board until you have consider-
                              WaveRunner Basic Orientation Video.  able practice and experience riding alone.
                              Showing them the video may help reinforce  Operating the watercraft with passengers
                              the information contained in these materi-  requires more skill. Take the time to be-
                              als.                                 come accustomed to the handling charac-
                                                                   teristics of the watercraft before trying any
                                                                   difficult maneuvers.

                            10

| 11 12 13 14 15 16 17 18 19 20 21 |