Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 8 - LIT-18626-12-58
P. 8

    UF2W16E0.book  Page 2  Monday, June 24, 2019  1:57 PM

                            General and important labels

                            EJU30353                              and page 52 for information on the removable
                              Emission control information
                                                                  watertight storage compartment.)
                            This engine conforms to U.S. Environmental
                            Protection Agency (EPA) and/or California Air
                            Resources Board (CARB) regulations for ma-
                            rine SI engines applicable at the time of man-
                            ufacture.
                            This engine is certified to operate on regular
                            unleaded gasoline.
                            EJU42511
                            Approval label of emission control
                            certificate                              1
                            This label is attached to the top of the cylin-
                                                                   1 Emission control information label location
                            der head and to the inside of the engine com-
                            partment. (See page 47 for seat removal and  EMISSION CONTROL INFORMATION
                                                                   THIS ENGINE CONFORMS TO          CALIFORNIA AND U.S. EPA EXHAUST REGULATIONS
                            installation procedures,  page 89  for engine  FOR SI MARINE ENGINES. REFER TO OWNER’S MANUAL FOR MAINTENANCE
                                                                   SPECIFICATIONS AND ADJUSTMENTS.
                                                                   ENGINE FAMILY :  DISPLACEMENT :                                            liters
                            cover removal  and installation procedures,  MAX POWER :                                    kW  EPA/CA FEL : HC+NOx            , CO            g/kW-h
                                                                   YAMAHA MOTOR CO.,LTD.
                                                                                        1

                                                                   1 Emission control information label location

                                                                               EPA/CA      ,
                                                                                 KNCNPLINEME2 ,   KYMXPTANKTK2 ,   KBEMPMDRN003
                                                                           KYMXPVSSLYM1
                                                                  EJU40491
                                                                  Manufactured date label
                                                                  This label is attached to the top of the cylin-
                                                                  der head. (See page 47 for seat removal and
                                                                  installation procedures and page 89 for en-

                            2

| 3 4 5 6 7 8 9 10 11 12 13 |