Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 65 - LIT-18626-12-61
P. 65

    UF3V11E0.book  Page 59  Tuesday, June 18, 2019  5:16 PM

                                                                     Equipment operation

                            To open the stern storage compartment:  the stern  storage  compartment while the
                            Unhook the stern storage compartment latch  rope is attached to the cleat.
                            on both sides, and then open the lid.

                                                                           1
                                                            1

                                                                   1 Ski rope slot
                              1 Stern storage compartment latch   EJU35175
                                                                  Beverage holder
                                                                  The beverage holder is located near the star-
                                            2                     board (right) side of the multifunction infor-
                                                          1       mation center.

                                                                                            1

                              1 Stern storage compartment lid
                              2 Stern storage compartment

                              Stern storage compartment:
                                Capacity:                          1 Beverage holder
                                  11.0 L (2.9 US gal, 2.4 Imp.gal)
                                Load limit:                       Do not place any items in the beverage hold-
                                  1.5 kg (3 lb)                   er while riding. Otherwise, the items may fall
                                                                  out of the beverage holder.
                            To close the stern storage compartment:  EJU37235
                                                                  Removable watertight storage compart-
                            Close the lid, and then hook the stern storage
                                                                  ment
                            compartment latch on both sides.
                                                                  The removable watertight storage compart-
                            TIP:                                  ment is located under the rear seat.
                            The ski rope slot in the stern storage com-  The compartment is watertight when the cap
                            partment lid can be used to store the rope in  is closed securely.

                                                                                                   59

| 60 61 62 63 64 65 66 67 68 69 70 |