Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 55 - LIT-18626-12-61
P. 55

    UF3V11E0.book  Page 49  Tuesday, June 18, 2019  5:16 PM

                                                                     Instrument operation

                            Fuel information (“Fuel Info”)         Selecting the display language
                                                                   Displaying the time since the last mainte-
                                                                   nance
                              1            5.4   Av MPG            Resetting the settings, trip information, and
                              2            1.4   Gal Used          fuel information
                              3            0.6   Gp H
                                            Trip Info                   PIN Settings  Display

                                                                           Unit      Language

                              1 Average fuel consumption per gallon or liter
                                                                         Wellness      Reset
                              2 Total fuel used
                              3 Fuel consumption per hour
                                  Item          Description
                                           Shows the average dis-  Changing the PIN (“PIN Settings”)
                               Average fuel
                               consumption   tance that was traveled by   The PIN can be changed to any 4-digit num-
                              per gallon or li-  the watercraft on 1.0 gal-  ber.
                                  ter*     lon or 1.0 liter of fuel since
                                           the item was last reset.
                                           Shows the total fuel that
                                           has been consumed by             PIN Settings
                              Total fuel used*  the engine in gallons or li-  0  0   0     0
                                           ters since the item was
                                           last reset.                    1    1     1     1
                                           Shows the current fuel
                              Fuel consump-                               2    2     2     2
                               tion per hour  consumption in gallons
                                           per hour or liters per hour.          Save
                            * Touch and hold this item to reset it.
                            EJU45170
                            Drive control mode screen “ ”
                                                                  To change the PIN:
                            The drive control mode screen  shows the
                                                                  (1) Input the current PIN, and then tap the
                            setting screen for the drive control mode in
                                                                     “Enter” button.
                            the center display. (See page 41 for informa-
                                                                  (2) Input the  new PIN, and then tap the
                            tion on the drive control mode.)
                                                                     “Save” button.
                            EJU45181
                            Setting menu screen “ ”               (3) Input the new PIN again, and then tap the
                            The setting menu screen shows a menu for  “Confirm Save” button.
                            accessing the screens for the following func-  Adjusting the display brightness and se-
                            tions.                                lecting the color setting (“Display”)
                             Changing the PIN                    The brightness of the display can be set with-
                             Adjusting the display brightness and se-  in a range from 1% to 100%.
                              lecting the color setting
                             Selecting the display units

                                                                                                   49

| 50 51 52 53 54 55 56 57 58 59 60 |