Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 93 - LIT-18626-12-62
P. 93

    UF3X11E0.book  Page 87  Thursday, July 4, 2019  2:27 PM

                                                                                      Operation

                            (4) Have the first passenger board using the  are securely holding on to the person in
                                same procedure as the operator, place  front of them or to the handgrip provided.
                                their feet on the floor of the footwell, and
                                securely hold on to the operator.

                                                                  (7) Attach the engine shut-off cord (lanyard)
                                                                     to your left wrist, and then attach the clip
                            (5) Have the second passenger  follow the  to the engine shut-off switch.
                                same procedure. When the second pas-  (8) Look  in all directions, start  the  engine,
                                senger is boarding,  try to  balance the  and then start off slowly.
                                watercraft together with the first passen-  EJU33084
                                                                  Starting off
                                ger.
                                                                  EWJ00713
                                                                      WARNING
                                                                  To avoid collisions:
                                                                   Scan constantly for people, objects, and
                                                                   other watercraft. Be alert for conditions
                                                                   that limit your visibility or block your vi-
                                                                   sion of others.
                                                                   Operate defensively at safe speeds and
                                                                   keep a safe distance away from people,
                                                                   objects, and other watercraft.
                                                                   Do not follow directly behind watercraft
                            (6) Make sure that  the passenger(s)  have
                                                                   or other boats. Do not go near others to
                                their feet on the floor of the footwell and
                                                                   spray or splash them with water, go too
                                                                   close to other boats, or go too fast for
                                                                   the traffic conditions. Avoid sharp turns
                                                                   or other maneuvers that make it hard for
                                                                   others to avoid you or understand where
                                                                   you are going.  Avoid areas with sub-
                                                                   merged objects or shallow water.
                                                                   Take early action to avoid collisions. Re-
                                                                   member, watercraft and other boats do
                                                                   not have  brakes. Do not  release  the
                                                                   throttle lever when trying to steer away

                                                                                                   87

| 88 89 90 91 92 93 94 95 96 97 98 |