Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 63 - LIT-18626-12-62
P. 63

    UF3X11E0.book  Page 57  Thursday, July 4, 2019  2:27 PM

                                                                     Equipment operation

                            could fall, which could result in severe in-  cleats break, the watercraft could fall,
                            jury. [EWJ01511]                      which could result in severe injury. [EWJ00822]
                                                                  FX Cruiser SVHO
                                                                                                1
                                    1

                              1 Cleat
                                                                   1 Pull-up cleat
                            EJU34894
                            Pull-up cleats (FX Cruiser SVHO / FX   FX Limited SVHO
                            Limited SVHO)                                                       1
                            The pull-up cleats are used to attach a rope
                            to the watercraft when mooring it.
                            To use a pull-up cleat, pull it up. The pull-up
                            cleat returns automatically to its original posi-
                            tion when released. WARNING! Do not use
                            the pull-up cleats to lift the watercraft. The
                            pull-up cleats are not designed to support
                            the watercraft’s weight. If the pull-up

                                                                   1 Pull-up cleat
                                                                  EJU35148
                                                                  Storage compartments
                                                                  This watercraft is equipped with the following
                                                                  storage compartments.
                                                                  Only the securely closed watertight storage
                                                                  compartment is waterproof. If you carry ob-
                                                                  jects that must be kept dry, put them in a wa-
                                                                  terproof bag.
                                                                  Make sure  that the storage  compartments
                                                                  are closed securely before operating the wa-
                                                                  tercraft.
                                                                  EJU45250
                                                                  Bow storage compartment
                                                                  The bow storage compartment is located un-
                                                                  der the hood.

                                                                                                   57

| 58 59 60 61 62 63 64 65 66 67 68 |