Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 56 - LIT-18626-12-63
P. 56

    UF4E14E0.book  Page 50  Wednesday, July 17, 2019  4:21 PM

                            Equipment operation

                            step  breaks,  the watercraft could fall,  EJU34873
                                                                  Bow eye
                            which could result in severe injury. [EWJ01212]
                                                                  The bow eye is used to attach a rope to the
                                                                  watercraft  when transporting, mooring, or
                                                                  towing it in an emergency. (See page 103 for
                                                                  information on towing the watercraft.)

                              1

                              1 Reboarding step
                                                                       1

                                                                   1 Bow eye
                                                                  EJU34882
                                                                  Stern eyes
                                                                  The stern eyes are used to attach a rope to
                                                                  the watercraft when transporting or mooring
                                                                  it.

                            ECJ00743
                             NOTICE
                            Use the reboarding step only to board the
                            watercraft in the water. Do not use the re-
                            boarding step for any other purpose. The
                            watercraft can be damaged.
                                                                           1

                                                                   1 Stern eye
                                                                  EJU40423
                                                                  Cleat
                                                                  The cleat is used to attach a ski rope to the
                                                                  watercraft  when pulling a wakeboarder or
                                                                  water-skier.  WARNING! Do not use the
                                                                  cleat to lift the watercraft. The cleat is not
                                                                  designed to support the watercraft’s
                                                                  weight. If the cleat breaks, the watercraft

                            50

| 51 52 53 54 55 56 57 58 59 60 61 |