Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 63 - LIT-18626-12-63
P. 63

    UF4E14E0.book  Page 57  Wednesday, July 17, 2019  4:21 PM

                                             Operation and handling requirements

                                curely closed before using  the  water-  EJU40291 Engine oil requirements
                                craft.
                                                                  EJU41514
                                                                  Engine oil
                                                                  ECJ00282
                                                                  NOTICE
                                                                  Use only 4-stroke engine oil. Usage of 2-
                                                                  stroke engine oil could result in severe en-
                                                                  gine damage.

                                                                    Recommended engine oil:
                                                                      YAMALUBE 4W or 4-stroke motor oil
                                                                    Recommended engine oil type:
                                                                      SAE 10W-30, 10W-40, 20W-40,
                            (11) Securely install the seats in their original  20W-50
                                positions.                          Recommended engine oil grade:
                                                                      API SG, SH, SJ, SL

                                                                  TIP:
                                                                  When the engine is operated at high speeds,
                                                                  some engine oil may be consumed. Be sure
                                                                  to check the engine oil level.
                                                                  Why Yamalube
                                                                  YAMALUBE oil is a Genuine YAMAHA Part
                                                                  born of the engineers’ passion and belief that
                                                                  engine oil is an important liquid engine com-
                                                                  ponent. We form teams of specialists in the
                                                                  fields of mechanical engineering, chemistry,
                                                                  electronics and track testing, and have them
                                                                  develop the engine together with the oil it will
                                                                  use. Yamalube oils take full advantage of the
                                                                  base oil’s qualities and blend in the ideal bal-
                                                                  ance of additives to make sure the final oil
                                                                  clears our performance standards. Thus,
                                                                  Yamalube mineral, semisynthetic and syn-
                                                                  thetic oils have their own distinct characters
                                                                  and value. Yamaha’s experience gained over
                                                                  many  years of  research and development
                                                                  into oil  since the 1960’s  helps  make

                                                                                                   57

| 58 59 60 61 62 63 64 65 66 67 68 |