Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 9 - LIT-18626-12-85
P. 9

    UF3X12E0.book  Page 3  Friday, May 22, 2020  10:00 AM

                                                          General and important labels

                            and page 60 for information on the removable  gine cover  removal and  installation proce-
                            watertight storage compartment.)      dures.)

                                                                         1

                                                 1

                              1 Emission control information label location  1 Manufactured date label location

                              EMISSION CONTROL INFORMATION
                              THIS ENGINE CONFORMS TO          CALIFORNIA AND U.S. EPA EXHAUST REGULATIONS
                              FOR SI MARINE ENGINES. REFER TO OWNER’S MANUAL FOR MAINTENANCE
                              SPECIFICATIONS AND ADJUSTMENTS.
                              ENGINE FAMILY :  DISPLACEMENT :                                            liters
                              MAX POWER :                                    kW  EPA/CA FEL : HC+NOx            , CO            g/kW-h
                              YAMAHA MOTOR CO.,LTD.
                                                1

                                                                  EJU30441
                                                                  Star labels
                                                                  This watercraft is labeled with a California Air
                                                                  Resources Board (CARB) star label. See be-
                              1 Emission control information label location  low for a description of your particular label.

                                                                                                 1

                                          EPA/CA      ,
                                           KNCNPLINEME2 ,   KYMXPTANKTK2 ,   KBEMPMDRN003
                                      KYMXPVSSLYM1
                            EJU40491
                            Manufactured date label
                            This label is attached to the top of the cylin-
                            der head. (See page 54 for seat removal and
                            installation procedures and page 96 for en-
                                                                   1 Star label location
                                                                  One Star - Low Emission
                                                                  The one-star label identifies engines that
                                                                  meet the Air Resources Board’s Personal

                                                                                                    3

| 4 5 6 7 8 9 10 11 12 13 14 |