Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 44 - LIT-18626-12-86
P. 44

    UF3V12E0.book  Page 38  Wednesday, June 3, 2020  2:38 PM

                            Watercraft operation

                                the bow. The trim angle can be adjusted  Vertical movement of the bow will be reduced
                                in the range of the trim settings –2 to +2.  and the watercraft will get up on plane more
                                                                  quickly when accelerating.

                                          1                         -2
                                              2
                              1 “TRIM/T.D.E.” up switch
                              2 “TRIM/T.D.E.” down switch
                            Bow-up positions
                            The bow will go up, causing the trim angle to
                            increase.
                            There is less water resistance, therefore,
                            straight-ahead acceleration is enhanced.

                              +2

                            Bow-down positions
                            The bow will go down, causing the trim angle
                            to decrease.

                            38

| 39 40 41 42 43 44 45 46 47 48 49 |