Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 53 - LIT-18626-12-87
P. 53

    UF3Y14E0.book  Page 47  Friday, June 12, 2020  10:50 AM

                                                                     Equipment operation

                            must be kept dry, put them in a waterproof  To close the bow storage compartment:
                            bag.                                  Return the hood to its original position, and
                            Make  sure that  the storage compartments  then hook the hood latches to secure it in pla-
                            are closed securely before operating the wa-  ce.
                            tercraft.
                            EJU44660
                            Bow storage compartment
                            The bow storage compartment is located un-
                            der the hood.
                            To open the bow storage compartment:
                            Unhook the hood latches, and then lift up the                      1
                            rear of the hood.

                                                                   1 Hood latch
                                                                  EJU43781
                                                                  Glove compartment
                                                         1        The glove compartment is located in front of
                                                                  the seat.

                              1 Hood latch

                                            1

                              1 Bow storage compartment
                              Bow storage compartment:
                                Capacity:
                                  7.0 L (1.8 US gal, 1.5 Imp.gal)
                                Load limit:
                                  2.0 kg (4 lb)

                                                                                                   47

| 48 49 50 51 52 53 54 55 56 57 58 |