Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 52 - LIT-18626-12-87
P. 52

    UF3Y14E0.book  Page 46  Friday, June 12, 2020  10:50 AM

                            Equipment operation

                            EJU34873                              could fall, which could result in severe in-
                            Bow eye
                                                                  jury. [EWJ01511]
                            The bow eye is used to attach a rope to the
                            watercraft when transporting, mooring, or
                            towing it in an emergency. (See page 96 for
                            information on towing the watercraft.)
                                                                                                1

                                                                   1 Cleat
                                                                  EJU34894
                                                                  Pull-up cleats (EX LIMITED)
                              1                                   The pull-up cleats are used to attach a rope
                              1 Bow eye
                                                                  to the watercraft when mooring it.
                            EJU34882                              To use a pull-up cleat, pull it up. The pull-up
                            Stern eyes                            cleat returns automatically to its original posi-
                            The stern eyes are used to attach a rope to
                                                                  tion when released. WARNING! Do not use
                            the watercraft when transporting or mooring
                                                                  the pull-up cleats to lift the watercraft. The
                            it.
                                                                  pull-up cleats are not designed to support
                                                                  the watercraft’s weight. If the pull-up
                                                                  cleats break, the watercraft could fall,
                                                                  which could result in severe injury. [EWJ00822]

                                                                                1

                               1
                              1 Stern eye
                            EJU40423
                            Cleat
                            The cleat is used to attach a ski rope to the
                            watercraft  when pulling a  wakeboarder or
                                                                   1 Pull-up cleat
                            water-skier.  WARNING!  Do not use the
                                                                  EJU31685
                            cleat to lift the watercraft. The cleat is not
                                                                  Storage compartments
                            designed to support the watercraft’s  This watercraft is equipped with the following
                            weight. If the cleat breaks, the watercraft  storage compartments.
                                                                  The storage compartments are not designed
                                                                  to be waterproof.  If you carry objects that

                            46

| 47 48 49 50 51 52 53 54 55 56 57 |