Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 57 - LIT-18626-12-88
P. 57

    UF4L12E0.book  Page 51  Thursday, June 4, 2020  2:02 PM

                                             Operation and handling requirements

                                and installation procedures and page 46  (9) Repeat steps 6–8 until the engine oil is at
                                for information on the seat storage com-  the proper level.
                                partment.)                        (10) Securely install the oil tank filler cap and
                            (6) Loosen the oil tank filler cap and remove  turn it until it stops.
                                it, and then wipe  the attached dipstick  (11) Securely install the seat  storage  com-
                                clean.                               partment and seat in their original posi-
                                                                     tions.

                                                            1

                              1 Oil tank filler cap/Dipstick
                            (7) Screw the oil tank filler cap into the filler
                                hole until it stops. Remove the oil tank
                                filler cap again and make sure that the
                                engine oil level is between the minimum
                                and maximum level marks.

                                    1    2      3

                              1 Dipstick
                              2 Maximum level mark
                              3 Minimum level mark
                            (8) If the  engine oil  level is significantly
                                above the maximum level mark, consult
                                a Yamaha dealer. If the engine oil level is
                                below the minimum  level  mark, slowly
                                add engine oil.

                                                                                                   51

| 52 53 54 55 56 57 58 59 60 61 62 |